Thankyou very much for you message, and I thought that I would let you know that your idea lead me to solving the play in the breaker plate. I used tin foil folded a number of times to make the thickness, then re assembled all the parts, Of course I imagine tin foil will not be all that durable, but it works for now and I have Plenty of the stuff. 

Now it will be interesting if this will have a positive effect on the pitting of the points. 

Thankyou very much for your help, it is sure comforting to know that there is a knowledge source available for advice. 

Thankyou so much. 

Talk to you again soon 

Regards Honda 600 owner
----- Original Message ----- From: william colford To: Honda 600 Owner Sent: Thursday, November 01, 2001 5:50 PM Subject: Re: I have a problem 

HI Owner; 

The breaker plate (where the points are bolted to) is not supposed to have any play. If yours does then you can search the junk yards, or, take it out, put it in a plastic bag, and take it apart. The plastic bag is important because it prevents you from losing the ball bearings in between the plates. What has happened is ... The silver colored plate sits on the dark blue or lower plate which has a shaft that it swings back and forth on. Some times you can turn the lower plate and there will be new (unworn) surface to ride on. But usually this is not the case. 
So the project is to replace the warn metal on the shaft so the upper (silver) plate swings back and forth without causing the points to lose the .016 clearance they are supposed to maintain. To do this, go to the local hardware store and purchase some one thousands stainless steel shim stock. Cut a 1/8 inch wide, 3in long strip from the shim stock and with the lower plate exposed force stainless steel shim stock into the area between the center shaft and the plate, allow the excess shim stock to lay on top of the plate. Now put everything back together, (apply some grease to the ball bearings).... adjust the points and everything should be ok 

r/Bill 
----- Original Message ----- 

